    PAD Specification File
    ***************************

    PART TYPE:        LCMXO2-1200HC
    Performance Grade:      4
    PACKAGE:          QFN32
    Package Status:                     Final          Version 1.44

    Mon Nov 22 17:19:06 2021

    Pinout by Port Name:
    +-----------+----------+--------------+-------+-----------+-----------+--------------------------------+
    | Port Name | Pin/Bank | Buffer Type  | Site  | PG Enable | BC Enable | Properties                     |
    +-----------+----------+--------------+-------+-----------+-----------+--------------------------------+
    | p2pin0    | 13/2     | LVCMOS25_OUT | PB11A |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin1    | 14/2     | LVCMOS25_OUT | PB11B |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin10   | 5/3      | LVCMOS25_OUT | PL9B  |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin11   | 8/2      | LVCMOS25_OUT | PB4C  |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin12   | 9/2      | LVCMOS25_OUT | PB6C  |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin13   | 10/2     | LVCMOS25_OUT | PB6D  |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin14   | 11/2     | LVCMOS25_OUT | PB9A  |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin15   | 12/2     | LVCMOS25_OUT | PB9B  |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin2    | 16/2     | LVCMOS25_OUT | PB20C |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin3    | 17/2     | LVCMOS25_OUT | PB20D |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin4    | 20/1     | LVCMOS25_OUT | PR5D  |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin5    | 21/1     | LVCMOS25_OUT | PR5C  |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin6    | 26/0     | LVCMOS25_OUT | PT15C |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin7    | 27/0     | LVCMOS25_OUT | PT12D |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin8    | 28/0     | LVCMOS25_OUT | PT12C |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | p2pin9    | 4/3      | LVCMOS25_OUT | PL9A  |           |           | DRIVE:8mA PULL:DOWN SLEW:SLOW  |
    | pin7_done | 23/0     | LVCMOS25_OUT | PT17D |           |           | DRIVE:8mA SLEW:SLOW            |
    | pin8_pgmn | 25/0     | LVCMOS25_OUT | PT15D |           |           | DRIVE:8mA SLEW:SLOW            |
    +-----------+----------+--------------+-------+-----------+-----------+--------------------------------+

    Vccio by Bank:
    +------+-------+
    | Bank | Vccio |
    +------+-------+
    | 0    | 2.5V  |
    | 1    | 2.5V  |
    | 2    | 2.5V  |
    | 3    | 2.5V  |
    +------+-------+

    Vref by Bank:
    +------+-----+-----------------+---------+
    | Vref | Pin | Bank # / Vref # | Load(s) |
    +------+-----+-----------------+---------+
    +------+-----+-----------------+---------+

    Pinout by Pin Number:
    +----------+-----------------------+------------+--------------+-------+---------------+-----------+-----------+
    | Pin/Bank | Pin Info              | Preference | Buffer Type  | Site  | Dual Function | PG Enable | BC Enable |
    +----------+-----------------------+------------+--------------+-------+---------------+-----------+-----------+
    | 1/0      | Reserved: sysCONFIG   |            |              | PT10C | TDO           |           |           |
    | 4/3      | p2pin9                | LOCATED    | LVCMOS25_OUT | PL9A  | PCLKT3_0      |           |           |
    | 5/3      | p2pin10               | LOCATED    | LVCMOS25_OUT | PL9B  | PCLKC3_0      |           |           |
    | 8/2      | p2pin11               | LOCATED    | LVCMOS25_OUT | PB4C  | CSSPIN        |           |           |
    | 9/2      | p2pin12               | LOCATED    | LVCMOS25_OUT | PB6C  | MCLK/CCLK     |           |           |
    | 10/2     | p2pin13               | LOCATED    | LVCMOS25_OUT | PB6D  | SO/SPISO      |           |           |
    | 11/2     | p2pin14               | LOCATED    | LVCMOS25_OUT | PB9A  | PCLKT2_0      |           |           |
    | 12/2     | p2pin15               | LOCATED    | LVCMOS25_OUT | PB9B  | PCLKC2_0      |           |           |
    | 13/2     | p2pin0                | LOCATED    | LVCMOS25_OUT | PB11A | PCLKT2_1      |           |           |
    | 14/2     | p2pin1                | LOCATED    | LVCMOS25_OUT | PB11B | PCLKC2_1      |           |           |
    | 16/2     | p2pin2                | LOCATED    | LVCMOS25_OUT | PB20C | SN            |           |           |
    | 17/2     | p2pin3                | LOCATED    | LVCMOS25_OUT | PB20D | SI/SISPI      |           |           |
    | 20/1     | p2pin4                | LOCATED    | LVCMOS25_OUT | PR5D  | PCLKC1_0/DQ0  |           |           |
    | 21/1     | p2pin5                | LOCATED    | LVCMOS25_OUT | PR5C  | PCLKT1_0/DQ0  |           |           |
    | 23/0     | pin7_done             | LOCATED    | LVCMOS25_OUT | PT17D | DONE          |           |           |
    | 25/0     | pin8_pgmn             | LOCATED    | LVCMOS25_OUT | PT15D | PROGRAMN      |           |           |
    | 26/0     | p2pin6                | LOCATED    | LVCMOS25_OUT | PT15C | JTAGENB       |           |           |
    | 27/0     | p2pin7                | LOCATED    | LVCMOS25_OUT | PT12D | SDA/PCLKC0_0  |           |           |
    | 28/0     | p2pin8                | LOCATED    | LVCMOS25_OUT | PT12C | SCL/PCLKT0_0  |           |           |
    | 29/0     | Reserved: sysCONFIG   |            |              | PT11D | TMS           |           |           |
    | 30/0     | Reserved: sysCONFIG   |            |              | PT11C | TCK           |           |           |
    | 32/0     | Reserved: sysCONFIG   |            |              | PT10D | TDI           |           |           |
    | PB4A/2   |     unused, PULL:DOWN |            |              | PB4A  |               |           |           |
    | PB4B/2   |     unused, PULL:DOWN |            |              | PB4B  |               |           |           |
    | PB4D/2   |     unused, PULL:DOWN |            |              | PB4D  |               |           |           |
    | PB6A/2   |     unused, PULL:DOWN |            |              | PB6A  |               |           |           |
    | PB6B/2   |     unused, PULL:DOWN |            |              | PB6B  |               |           |           |
    | PB9C/2   |     unused, PULL:DOWN |            |              | PB9C  |               |           |           |
    | PB9D/2   |     unused, PULL:DOWN |            |              | PB9D  |               |           |           |
    | PB11C/2  |     unused, PULL:DOWN |            |              | PB11C |               |           |           |
    | PB11D/2  |     unused, PULL:DOWN |            |              | PB11D |               |           |           |
    | PB15A/2  |     unused, PULL:DOWN |            |              | PB15A |               |           |           |
    | PB15B/2  |     unused, PULL:DOWN |            |              | PB15B |               |           |           |
    | PB15C/2  |     unused, PULL:DOWN |            |              | PB15C |               |           |           |
    | PB15D/2  |     unused, PULL:DOWN |            |              | PB15D |               |           |           |
    | PB18A/2  |     unused, PULL:DOWN |            |              | PB18A |               |           |           |
    | PB18B/2  |     unused, PULL:DOWN |            |              | PB18B |               |           |           |
    | PB18C/2  |     unused, PULL:DOWN |            |              | PB18C |               |           |           |
    | PB18D/2  |     unused, PULL:DOWN |            |              | PB18D |               |           |           |
    | PB20A/2  |     unused, PULL:DOWN |            |              | PB20A |               |           |           |
    | PB20B/2  |     unused, PULL:DOWN |            |              | PB20B |               |           |           |
    | PL2A/3   |     unused, PULL:DOWN |            |              | PL2A  | L_GPLLT_FB    |           |           |
    | PL2B/3   |     unused, PULL:DOWN |            |              | PL2B  | L_GPLLC_FB    |           |           |
    | PL2C/3   |     unused, PULL:DOWN |            |              | PL2C  | L_GPLLT_IN    |           |           |
    | PL2D/3   |     unused, PULL:DOWN |            |              | PL2D  | L_GPLLC_IN    |           |           |
    | PL3A/3   |     unused, PULL:DOWN |            |              | PL3A  | PCLKT3_2      |           |           |
    | PL3B/3   |     unused, PULL:DOWN |            |              | PL3B  | PCLKC3_2      |           |           |
    | PL3C/3   |     unused, PULL:DOWN |            |              | PL3C  |               |           |           |
    | PL3D/3   |     unused, PULL:DOWN |            |              | PL3D  |               |           |           |
    | PL4A/3   |     unused, PULL:DOWN |            |              | PL4A  |               |           |           |
    | PL4B/3   |     unused, PULL:DOWN |            |              | PL4B  |               |           |           |
    | PL4C/3   |     unused, PULL:DOWN |            |              | PL4C  |               |           |           |
    | PL4D/3   |     unused, PULL:DOWN |            |              | PL4D  |               |           |           |
    | PL5A/3   |     unused, PULL:DOWN |            |              | PL5A  | PCLKT3_1      |           |           |
    | PL5B/3   |     unused, PULL:DOWN |            |              | PL5B  | PCLKC3_1      |           |           |
    | PL5C/3   |     unused, PULL:DOWN |            |              | PL5C  |               |           |           |
    | PL5D/3   |     unused, PULL:DOWN |            |              | PL5D  |               |           |           |
    | PL8A/3   |     unused, PULL:DOWN |            |              | PL8A  |               |           |           |
    | PL8B/3   |     unused, PULL:DOWN |            |              | PL8B  |               |           |           |
    | PL8C/3   |     unused, PULL:DOWN |            |              | PL8C  |               |           |           |
    | PL8D/3   |     unused, PULL:DOWN |            |              | PL8D  |               |           |           |
    | PL10A/3  |     unused, PULL:DOWN |            |              | PL10A |               |           |           |
    | PL10B/3  |     unused, PULL:DOWN |            |              | PL10B |               |           |           |
    | PL10C/3  |     unused, PULL:DOWN |            |              | PL10C |               |           |           |
    | PL10D/3  |     unused, PULL:DOWN |            |              | PL10D |               |           |           |
    | PR2A/1   |     unused, PULL:DOWN |            |              | PR2A  | DQ0           |           |           |
    | PR2B/1   |     unused, PULL:DOWN |            |              | PR2B  | DQ0           |           |           |
    | PR2C/1   |     unused, PULL:DOWN |            |              | PR2C  | DQ0           |           |           |
    | PR2D/1   |     unused, PULL:DOWN |            |              | PR2D  | DQ0           |           |           |
    | PR3A/1   |     unused, PULL:DOWN |            |              | PR3A  | DQ0           |           |           |
    | PR3B/1   |     unused, PULL:DOWN |            |              | PR3B  | DQ0           |           |           |
    | PR4A/1   |     unused, PULL:DOWN |            |              | PR4A  | DQ0           |           |           |
    | PR4B/1   |     unused, PULL:DOWN |            |              | PR4B  | DQ0           |           |           |
    | PR4C/1   |     unused, PULL:DOWN |            |              | PR4C  | DQ0           |           |           |
    | PR4D/1   |     unused, PULL:DOWN |            |              | PR4D  | DQ0           |           |           |
    | PR5A/1   |     unused, PULL:DOWN |            |              | PR5A  | DQS0          |           |           |
    | PR5B/1   |     unused, PULL:DOWN |            |              | PR5B  | DQS0N         |           |           |
    | PR8A/1   |     unused, PULL:DOWN |            |              | PR8A  | DQS1          |           |           |
    | PR8B/1   |     unused, PULL:DOWN |            |              | PR8B  | DQS1N         |           |           |
    | PR8C/1   |     unused, PULL:DOWN |            |              | PR8C  | DQ1           |           |           |
    | PR8D/1   |     unused, PULL:DOWN |            |              | PR8D  | DQ1           |           |           |
    | PR9A/1   |     unused, PULL:DOWN |            |              | PR9A  | DQ1           |           |           |
    | PR9B/1   |     unused, PULL:DOWN |            |              | PR9B  | DQ1           |           |           |
    | PR9C/1   |     unused, PULL:DOWN |            |              | PR9C  | DQ1           |           |           |
    | PR9D/1   |     unused, PULL:DOWN |            |              | PR9D  | DQ1           |           |           |
    | PR10A/1  |     unused, PULL:DOWN |            |              | PR10A | DQ1           |           |           |
    | PR10B/1  |     unused, PULL:DOWN |            |              | PR10B | DQ1           |           |           |
    | PR10C/1  |     unused, PULL:DOWN |            |              | PR10C | DQ1           |           |           |
    | PR10D/1  |     unused, PULL:DOWN |            |              | PR10D | DQ1           |           |           |
    | PT9A/0   |     unused, PULL:DOWN |            |              | PT9A  |               |           |           |
    | PT9B/0   |     unused, PULL:DOWN |            |              | PT9B  |               |           |           |
    | PT9C/0   |     unused, PULL:DOWN |            |              | PT9C  |               |           |           |
    | PT9D/0   |     unused, PULL:DOWN |            |              | PT9D  |               |           |           |
    | PT10A/0  |     unused, PULL:DOWN |            |              | PT10A |               |           |           |
    | PT10B/0  |     unused, PULL:DOWN |            |              | PT10B |               |           |           |
    | PT11A/0  |     unused, PULL:DOWN |            |              | PT11A |               |           |           |
    | PT11B/0  |     unused, PULL:DOWN |            |              | PT11B |               |           |           |
    | PT12A/0  |     unused, PULL:DOWN |            |              | PT12A | PCLKT0_1      |           |           |
    | PT12B/0  |     unused, PULL:DOWN |            |              | PT12B | PCLKC0_1      |           |           |
    | PT15A/0  |     unused, PULL:DOWN |            |              | PT15A |               |           |           |
    | PT15B/0  |     unused, PULL:DOWN |            |              | PT15B |               |           |           |
    | PT16A/0  |     unused, PULL:DOWN |            |              | PT16A |               |           |           |
    | PT16B/0  |     unused, PULL:DOWN |            |              | PT16B |               |           |           |
    | PT16C/0  |     unused, PULL:DOWN |            |              | PT16C |               |           |           |
    | PT16D/0  |     unused, PULL:DOWN |            |              | PT16D |               |           |           |
    | PT17A/0  |     unused, PULL:DOWN |            |              | PT17A |               |           |           |
    | PT17B/0  |     unused, PULL:DOWN |            |              | PT17B |               |           |           |
    | PT17C/0  |     unused, PULL:DOWN |            |              | PT17C | INITN         |           |           |
    +----------+-----------------------+------------+--------------+-------+---------------+-----------+-----------+

    sysCONFIG Pins:
    +----------+--------------------+--------------------+----------+-------------+-------------------+
    | Pad Name | sysCONFIG Pin Name | sysCONFIG Settings | Pin/Bank | Buffer Type | Config Pull Mode  |
    +----------+--------------------+--------------------+----------+-------------+-------------------+
    | PT11D    | TMS                | JTAG_PORT=ENABLE   | 29/0     |             | PULLUP            |
    | PT11C    | TCK/TEST_CLK       | JTAG_PORT=ENABLE   | 30/0     |             | NO pull up/down   |
    | PT10D    | TDI/MD7            | JTAG_PORT=ENABLE   | 32/0     |             | PULLUP            |
    | PT10C    | TDO                | JTAG_PORT=ENABLE   | 1/0      |             | PULLUP            |
    +----------+--------------------+--------------------+----------+-------------+-------------------+

    Dedicated sysCONFIG Pins:

    List of All Pins' Locate Preferences Based on Final Placement After PAR
    to Help Users Lock Down ALL the Pins Easily (by Simply Copy & Paste):

    LOCATE  COMP  "p2pin0"  SITE  "13";
    LOCATE  COMP  "p2pin1"  SITE  "14";
    LOCATE  COMP  "p2pin10"  SITE  "5";
    LOCATE  COMP  "p2pin11"  SITE  "8";
    LOCATE  COMP  "p2pin12"  SITE  "9";
    LOCATE  COMP  "p2pin13"  SITE  "10";
    LOCATE  COMP  "p2pin14"  SITE  "11";
    LOCATE  COMP  "p2pin15"  SITE  "12";
    LOCATE  COMP  "p2pin2"  SITE  "16";
    LOCATE  COMP  "p2pin3"  SITE  "17";
    LOCATE  COMP  "p2pin4"  SITE  "20";
    LOCATE  COMP  "p2pin5"  SITE  "21";
    LOCATE  COMP  "p2pin6"  SITE  "26";
    LOCATE  COMP  "p2pin7"  SITE  "27";
    LOCATE  COMP  "p2pin8"  SITE  "28";
    LOCATE  COMP  "p2pin9"  SITE  "4";
    LOCATE  COMP  "pin7_done"  SITE  "23";
    LOCATE  COMP  "pin8_pgmn"  SITE  "25";

    PAR: Place And Route Diamond (64-bit) 3.12.1.454.
    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995 AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems   All rights reserved.
    Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.
    Mon Nov 22 17:19:06 2021