    BITGEN: Bitstream Generator Diamond (64-bit) 3.12.1.454
    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995 AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems   All rights reserved.
    Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.
    Mon Nov 22 17:19:22 2021

    Command: bitgen -g RamCfg:Reset -path C:/FPGA/4BitProject -w -jedec -gui -msgset C:/FPGA/4BitProject/promote.xml 4Bit_P2_a2_impl.ncd 4Bit_P2_a2_impl.prf

    Loading design for application Bitgen from file 4Bit_P2_a2_impl.ncd.
    Design name: TinyFPGA_A2
    NCD version: 3.3
    Vendor:      LATTICE
    Device:      LCMXO2-1200HC
    Package:     QFN32
    Performance: 4
    Loading device for application Bitgen from file 'xo2c1200.nph' in environment: C:/lscc/diamond/3.12/ispfpga.
    Package Status:                     Final          Version 1.44.
    Performance Hardware Data Status:   Final          Version 34.4.

    Running DRC.
    INFO: Design contains EBR with ASYNC Reset Mode that has a limitation: The use of the EBR block asynchronous reset requires that certain timing be met between the clock and the reset within the memory block. See the device specific data sheet for additional details.
    INFO: Design contains pre-loadable EBR during configuration that has a requirement: Since the GSR is disabled for the EBR, make sure write enable and chip enable are inactive during wake-up, so that the pre-loaded initialization values will not be corrupted during wake-up state.
    DRC detected 0 errors and 0 warnings.
    Reading Preference File from 4Bit_P2_a2_impl.prf.

    Preference Summary:

    +---------------------------------+---------------------------------+
    |  Preference                     |  Current Setting                |
    +---------------------------------+---------------------------------+
    |                         RamCfg  |                        Reset**  |
    +---------------------------------+---------------------------------+
    |                     MCCLK_FREQ  |                         2.08**  |
    +---------------------------------+---------------------------------+
    |                  CONFIG_SECURE  |                          OFF**  |
    +---------------------------------+---------------------------------+
    |                          INBUF  |                           ON**  |
    +---------------------------------+---------------------------------+
    |                      JTAG_PORT  |                       ENABLE**  |
    +---------------------------------+---------------------------------+
    |                       SDM_PORT  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
    |                 SLAVE_SPI_PORT  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
    |                MASTER_SPI_PORT  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
    |                       I2C_PORT  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
    |        MUX_CONFIGURATION_PORTS  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
    |                  CONFIGURATION  |                          CFG**  |
    +---------------------------------+---------------------------------+
    |                COMPRESS_CONFIG  |                           ON**  |
    +---------------------------------+---------------------------------+
    |                        MY_ASSP  |                          OFF**  |
    +---------------------------------+---------------------------------+
    |               ONE_TIME_PROGRAM  |                          OFF**  |
    +---------------------------------+---------------------------------+
    |                 ENABLE_TRANSFR  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
    |                  SHAREDEBRINIT  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
    |            BACKGROUND_RECONFIG  |                          OFF**  |
    +---------------------------------+---------------------------------+
     *  Default setting.
     ** The specified setting matches the default setting.

    Creating bit map...

    Bitstream Status: Final           Version 1.95.

    Saving bit stream in "4Bit_P2_a2_impl.jed".

    ===========
    UFM Summary.
    ===========
    UFM Size:        511 Pages (128*511 Bits).
    UFM Utilization: General Purpose Flash Memory.

    Available General Purpose Flash Memory:  511 Pages (Page 0 to Page 510).
    Initialized UFM Pages:                     0 Page.

    Total CPU Time: 6 secs
    Total REAL Time: 7 secs
    Peak Memory Usage: 257 MB