             Lattice Mapping Report File for Design Module 'TinyFPGA_A2'

    Design Information

    Command line:   map -a MachXO2 -p LCMXO2-1200HC -t QFN32 -s 4 -oc Commercial
         4Bit_P2_a2_impl.ngd -o 4Bit_P2_a2_impl_map.ncd -pr 4Bit_P2_a2_impl.prf -mp
         4Bit_P2_a2_impl.mrp -lpf C:/FPGA/4BitProject/impl/4Bit_P2_a2_impl.lpf -lpf
         C:/FPGA/4BitProject/template_P2_a2.lpf -c 0 -gui -msgset
         C:/FPGA/4BitProject/promote.xml
    Target Vendor:  LATTICE
    Target Device:  LCMXO2-1200HCQFN32
    Target Performance:   4
    Mapper:  xo2c00,  version:  Diamond (64-bit) 3.12.1.454
    Mapped on:  11/23/21  15:00:58

    Design Summary
       Number of registers:     82 out of  1346 (6%)
          PFU registers:           82 out of  1280 (6%)
          PIO registers:            0 out of    66 (0%)
       Number of SLICEs:       629 out of   640 (98%)
          SLICEs as Logic/ROM:    629 out of   640 (98%)
          SLICEs as RAM:            0 out of   480 (0%)
          SLICEs as Carry:         34 out of   640 (5%)
       Number of LUT4s:        1255 out of  1280 (98%)
          Number used as logic LUTs:        1187
          Number used as distributed RAM:     0
          Number used as ripple logic:       68
          Number used as shift registers:     0
       Number of PIO sites used: 18 + 4(JTAG) out of 22 (100%)
       Number of block RAMs:  4 out of 7 (57%)
       Number of GSRs:        0 out of 1 (0%)
       EFB used :        No
       JTAG used :       No
       Readback used :   No
       Oscillator used : Yes
       Startup used :    No
       POR :             On
       Bandgap :         On
       Number of Power Controller:  0 out of 1 (0%)
       Number of Dynamic Bank Controller (BCINRD):  0 out of 4 (0%)
       Number of Dynamic Bank Controller (BCLVDSO):  0 out of 1 (0%)
       Number of DCCA:  0 out of 8 (0%)
       Number of DCMA:  0 out of 2 (0%)
       Number of PLLs:  0 out of 1 (0%)
       Number of DQSDLLs:  0 out of 2 (0%)
       Number of CLKDIVC:  0 out of 4 (0%)
       Number of ECLKSYNCA:  0 out of 4 (0%)
       Number of ECLKBRIDGECS:  0 out of 2 (0%)
       Notes:-
          1. Total number of LUT4s = (Number of logic LUT4s) + 2*(Number of
         distributed RAMs) + 2*(Number of ripple logic)
          2. Number of logic LUT4s does not include count of distributed RAM and
         ripple logic.
       Number of clocks:  2
         Net clk: 30 loads, 30 rising, 0 falling (Driver: internal_oscillator_inst )

         Net p2pin13_c_17: 21 loads, 21 rising, 0 falling (Driver: led_timer_95__i17

         )
       Number of Clock Enables:  5
         Net PHASE: 4 loads, 4 LSLICEs
         Net EBR_ROM_IP2_inst/Microcode1_Output_4: 1 loads, 1 LSLICEs
         Net EBR_ROM_IP2_inst/Microcode1_Output_5: 3 loads, 3 LSLICEs
         Net QuadD_74173_inst3/Q_3_N_179_0: 2 loads, 2 LSLICEs
         Net QuadD_74173_inst4/Q_3_N_179_0: 2 loads, 2 LSLICEs
       Number of LSRs:  2
         Net RESETn: 8 loads, 8 LSLICEs
         Net Program_Address_11: 6 loads, 6 LSLICEs
       Number of nets driven by tri-state buffers:  0
       Top 10 highest fanout non-clock nets:
         Net Program_Address_3: 664 loads
         Net p2pin12_c_0: 518 loads
         Net Program_Address_1: 474 loads
         Net Program_Address_2: 454 loads
         Net Program_Address_4: 445 loads
         Net Program_Address_5: 237 loads
         Net Program_Address_6: 117 loads
         Net Program_Address_7: 59 loads
         Net Program_Address_8: 35 loads
         Net n340: 29 loads

       Number of warnings:  3
       Number of errors:    0

    Design Errors/Warnings

    WARNING - map: Converting L6MUX21 i6753/GATE to normal MUX21.
    WARNING - map: Converting L6MUX21 i6756/GATE to normal MUX21.
    WARNING - map: Converted 2 L6MUX21's to normal MUX21.

    IO (PIO) Attributes

    +---------------------+-----------+-----------+------------+
    | IO Name             | Direction | Levelmode | IO         |
    |                     |           |  IO_TYPE  | Register   |
    +---------------------+-----------+-----------+------------+
    | p2pin0              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin1              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin2              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin3              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin4              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin5              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+

    | pin7_done           | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | pin8_pgmn           | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin6              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin7              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin12             | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin13             | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin14             | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin15             | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin8              | INPUT     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin9              | INPUT     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin10             | INPUT     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | p2pin11             | INPUT     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+

    Removed logic

    Block GSR_INST undriven or does not drive anything - clipped.
    Signal p2pin13_c_17_enable_13 was merged into signal
         EBR_ROM_IP2_inst/Microcode1_Output_5
    Signal p2pin13_c_17_enable_14 was merged into signal
         EBR_ROM_IP2_inst/Microcode1_Output_4
    Signal n4431 was merged into signal RESETn
    Signal p2pin13_c_17_enable_10 was merged into signal PHASE
    Signal Microcode0_Output_4__N_46 was merged into signal Microcode0_Output_4
    Signal VCC_net undriven or does not drive anything - clipped.
    Signal add_5673_13/S1 undriven or does not drive anything - clipped.
    Signal add_5673_13/S0 undriven or does not drive anything - clipped.
    Signal led_timer_95_add_4_33/S1 undriven or does not drive anything - clipped.
    Signal led_timer_95_add_4_33/CO undriven or does not drive anything - clipped.
    Signal add_5673_15/S1 undriven or does not drive anything - clipped.
    Signal add_5673_15/S0 undriven or does not drive anything - clipped.
    Signal add_5673_1/S1 undriven or does not drive anything - clipped.
    Signal add_5673_1/S0 undriven or does not drive anything - clipped.
    Signal add_5673_1/CI undriven or does not drive anything - clipped.
    Signal add_5673_17/S1 undriven or does not drive anything - clipped.
    Signal add_5673_17/S0 undriven or does not drive anything - clipped.
    Signal add_5673_3/S1 undriven or does not drive anything - clipped.
    Signal add_5673_3/S0 undriven or does not drive anything - clipped.
    Signal add_5673_19/S1 undriven or does not drive anything - clipped.
    Signal add_5673_19/S0 undriven or does not drive anything - clipped.
    Signal add_5673_21/S1 undriven or does not drive anything - clipped.
    Signal add_5673_21/S0 undriven or does not drive anything - clipped.
    Signal add_5673_5/S1 undriven or does not drive anything - clipped.
    Signal add_5673_5/S0 undriven or does not drive anything - clipped.

    Signal add_5673_23/S1 undriven or does not drive anything - clipped.
    Signal add_5673_23/S0 undriven or does not drive anything - clipped.
    Signal add_5673_25/S1 undriven or does not drive anything - clipped.
    Signal add_5673_25/S0 undriven or does not drive anything - clipped.
    Signal add_5673_27/S1 undriven or does not drive anything - clipped.
    Signal add_5673_27/S0 undriven or does not drive anything - clipped.
    Signal add_5673_29/S1 undriven or does not drive anything - clipped.
    Signal add_5673_29/S0 undriven or does not drive anything - clipped.
    Signal add_5673_31/S1 undriven or does not drive anything - clipped.
    Signal add_5673_31/S0 undriven or does not drive anything - clipped.
    Signal add_5673_33/S0 undriven or does not drive anything - clipped.
    Signal add_5673_33/CO undriven or does not drive anything - clipped.
    Signal led_timer_95_add_4_1/S0 undriven or does not drive anything - clipped.
    Signal led_timer_95_add_4_1/CI undriven or does not drive anything - clipped.
    Signal add_5673_7/S1 undriven or does not drive anything - clipped.
    Signal add_5673_7/S0 undriven or does not drive anything - clipped.
    Signal add_5673_9/S1 undriven or does not drive anything - clipped.
    Signal add_5673_9/S0 undriven or does not drive anything - clipped.
    Signal add_5673_11/S1 undriven or does not drive anything - clipped.
    Signal add_5673_11/S0 undriven or does not drive anything - clipped.
    Block EBR_ROM_IP2_inst/i4165_1_lut was optimized away.
    Block EBR_ROM_IP2_inst/i4164_1_lut was optimized away.
    Block i4172_1_lut was optimized away.
    Block i4168_1_lut was optimized away.
    Block Microcode0_Output_4__I_0_1_lut was optimized away.
    Block i2 was optimized away.

    Memory Usage

    /EBR_RAM_DQ_IP_inst:
        EBRs: 2
        RAM SLICEs: 0
        Logic SLICEs: 0
        PFU Registers: 0
        -Contains EBR EBR_RAM_DQ_IP_0_1_0:  TYPE= DP8KC,  Width_A= 2,  Depth_A=
             4096,  REGMODE_A= OUTREG,  REGMODE_B= NOREG,  RESETMODE= SYNC,
             ASYNC_RESET_RELEASE= SYNC,  WRITEMODE_A= NORMAL,  WRITEMODE_B= NORMAL,
             GSR= DISABLED,  MEM_INIT_FILE= INIT_ALL_0s,  MEM_LPC_FILE=
             EBR_RAM_DQ_IP.lpc
        -Contains EBR EBR_RAM_DQ_IP_0_0_1:  TYPE= DP8KC,  Width_A= 2,  Depth_A=
             4096,  REGMODE_A= OUTREG,  REGMODE_B= NOREG,  RESETMODE= SYNC,
             ASYNC_RESET_RELEASE= SYNC,  WRITEMODE_A= NORMAL,  WRITEMODE_B= NORMAL,
             GSR= DISABLED,  MEM_INIT_FILE= INIT_ALL_0s,  MEM_LPC_FILE=
             EBR_RAM_DQ_IP.lpc
    /EBR_ROM_IP2_inst:
        EBRs: 1
        RAM SLICEs: 0
        Logic SLICEs: 0
        PFU Registers: 0
        -Contains EBR EBR_ROM_IP2_0_0_0:  TYPE= DP8KC,  Width_A= 8,  Depth_A= 128,
             REGMODE_A= OUTREG,  REGMODE_B= NOREG,  RESETMODE= SYNC,
             ASYNC_RESET_RELEASE= SYNC,  WRITEMODE_A= NORMAL,  WRITEMODE_B= NORMAL,
             GSR= DISABLED,  MEM_INIT_FILE= microcode_1.mem,  MEM_LPC_FILE=
             EBR_ROM_IP2.lpc
    /EBR_ROM_IP_inst:

        EBRs: 1
        RAM SLICEs: 0
        Logic SLICEs: 0
        PFU Registers: 0
        -Contains EBR EBR_ROM_IP_0_0_0:  TYPE= DP8KC,  Width_A= 8,  Depth_A= 128,
             REGMODE_A= OUTREG,  REGMODE_B= NOREG,  RESETMODE= SYNC,
             ASYNC_RESET_RELEASE= SYNC,  WRITEMODE_A= NORMAL,  WRITEMODE_B= NORMAL,
             GSR= DISABLED,  MEM_INIT_FILE= microcode_0.mem,  MEM_LPC_FILE=
             EBR_ROM_IP.lpc

    OSC Summary
    -----------

    OSC 1:                                     Pin/Node Value
      OSC Instance Name:                                internal_oscillator_inst
      OSC Type:                                         OSCH
      STDBY Input:                                      NONE
      OSC Output:                              NODE     clk
      OSC Nominal Frequency (MHz):                      2.08

    ASIC Components
    ---------------

    Instance Name: internal_oscillator_inst
             Type: OSCH
    Instance Name: EBR_RAM_DQ_IP_inst/EBR_RAM_DQ_IP_0_1_0
             Type: DP8KC
    Instance Name: EBR_RAM_DQ_IP_inst/EBR_RAM_DQ_IP_0_0_1
             Type: DP8KC
    Instance Name: EBR_ROM_IP2_inst/EBR_ROM_IP2_0_0_0
             Type: DP8KC
    Instance Name: EBR_ROM_IP_inst/EBR_ROM_IP_0_0_0
             Type: DP8KC

    Run Time and Memory Usage
    -------------------------

       Total CPU Time: 2 secs
       Total REAL Time: 2 secs
       Peak Memory Usage: 47 MB

    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
         Copyright (c) 1995 AT&T Corp.   All rights reserved.
         Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
         Copyright (c) 2001 Agere Systems   All rights reserved.
         Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights
         reserved.