    PAD Specification File
    ***************************

    PART TYPE:        LFE5U-12F
    Performance Grade:      6
    PACKAGE:          CABGA381
    Package Status:                     Final          Version 1.42

    Sun Dec 05 13:18:12 2021

    Pinout by Port Name:
    +---------------+----------+---------------+-------+-----------+---------------------------------+
    | Port Name     | Pin/Bank | Buffer Type   | Site  | BC Enable | Properties                      |
    +---------------+----------+---------------+-------+-----------+---------------------------------+
    | btn[0]        | D6/0     | LVCMOS33_IN   | PT6B  |           | PULL:UP CLAMP:ON HYSTERESIS:ON  |
    | clk_25mhz     | G2/6     | LVCMOS33_IN   | PL26A |           | CLAMP:ON HYSTERESIS:ON          |
    | gpdi_dp[0]    | A16/1    | LVCMOS33D_OUT | PT56A |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | gpdi_dp[1]    | A14/1    | LVCMOS33D_OUT | PT47A |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | gpdi_dp[2]    | A12/1    | LVCMOS33D_OUT | PT40A |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | gpdi_dp[3]    | A17/1    | LVCMOS33D_OUT | PT62A |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | led[0]        | B2/7     | LVCMOS33_OUT  | PL14C |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | led[1]        | C2/7     | LVCMOS33_OUT  | PL14D |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | led[2]        | C1/7     | LVCMOS33_OUT  | PL17A |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | led[3]        | D2/7     | LVCMOS33_OUT  | PL17C |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | led[4]        | D1/7     | LVCMOS33_OUT  | PL17B |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | led[5]        | E2/7     | LVCMOS33_OUT  | PL23D |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | led[6]        | E1/7     | LVCMOS33_OUT  | PL17D |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | led[7]        | H3/7     | LVCMOS33_OUT  | PL20D |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | user_programn | M4/6     | LVCMOS33_OUT  | PL38A |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    | wifi_gpio0    | L2/6     | LVCMOS33_OUT  | PL41D |           | DRIVE:4mA CLAMP:ON SLEW:SLOW    |
    +---------------+----------+---------------+-------+-----------+---------------------------------+

    Vccio by Bank:
    +------+-------+
    | Bank | Vccio |
    +------+-------+
    | 0    | 3.3V  |
    | 1    | 3.3V  |
    | 6    | 3.3V  |
    | 7    | 3.3V  |
    | 8    | 3.3V  |
    +------+-------+

    Vref by Bank:
    +------+-----+-----------------+---------+
    | Vref | Pin | Bank # / Vref # | Load(s) |
    +------+-----+-----------------+---------+
    +------+-----+-----------------+---------+

    Pinout by Pin Number:
    +----------+-----------------------+------------+---------------+-------+--------------------------+-----------+
    | Pin/Bank | Pin Info              | Preference | Buffer Type   | Site  | Dual Function            | BC Enable |
    +----------+-----------------------+------------+---------------+-------+--------------------------+-----------+
    | A2/7     |     unused, PULL:DOWN |            |               | PL14A | LDQ20                    |           |
    | A3/7     |     unused, PULL:DOWN |            |               | PL5C  | LDQ8                     |           |
    | A4/7     |     unused, PULL:DOWN |            |               | PL2A  | LDQ8                     |           |
    | A5/7     |     unused, PULL:DOWN |            |               | PL2B  | LDQ8                     |           |
    | A6/0     |     unused, PULL:DOWN |            |               | PT4A  |                          |           |
    | A7/0     |     unused, PULL:DOWN |            |               | PT18A |                          |           |
    | A8/0     |     unused, PULL:DOWN |            |               | PT18B |                          |           |
    | A9/0     |     unused, PULL:DOWN |            |               | PT24A | GR_PCLK0_1               |           |
    | A10/0    |     unused, PULL:DOWN |            |               | PT27A | PCLKT0_1                 |           |
    | A11/0    |     unused, PULL:DOWN |            |               | PT27B |                          |           |
    | A12/1    | gpdi_dp[2]+           | LOCATED    | LVCMOS33D_OUT | PT40A |                          |           |
    | A13/1    | gpdi_dp[2]-           |            | LVCMOS33D_OUT | PT40B |                          |           |
    | A14/1    | gpdi_dp[1]+           | LOCATED    | LVCMOS33D_OUT | PT47A |                          |           |
    | A16/1    | gpdi_dp[0]+           | LOCATED    | LVCMOS33D_OUT | PT56A |                          |           |
    | A17/1    | gpdi_dp[3]+           | LOCATED    | LVCMOS33D_OUT | PT62A |                          |           |
    | A18/1    |     unused, PULL:DOWN |            |               | PT65A |                          |           |
    | A19/1    |     unused, PULL:DOWN |            |               | PT67A |                          |           |
    | B1/7     |     unused, PULL:DOWN |            |               | PL14B | LDQ20                    |           |
    | B2/7     | led[0]                | LOCATED    | LVCMOS33_OUT  | PL14C | VREF1_7/LDQ20            |           |
    | B3/7     |     unused, PULL:DOWN |            |               | PL5D  | LDQ8                     |           |
    | B4/7     |     unused, PULL:DOWN |            |               | PL5B  | LDQ8                     |           |
    | B5/7     |     unused, PULL:DOWN |            |               | PL2C  | LDQ8                     |           |
    | B6/0     |     unused, PULL:DOWN |            |               | PT4B  |                          |           |
    | B8/0     |     unused, PULL:DOWN |            |               | PT15B |                          |           |
    | B9/0     |     unused, PULL:DOWN |            |               | PT22A |                          |           |
    | B10/0    |     unused, PULL:DOWN |            |               | PT24B | GR_PCLK0_0               |           |
    | B11/0    |     unused, PULL:DOWN |            |               | PT29A | PCLKT0_0                 |           |
    | B12/1    |     unused, PULL:DOWN |            |               | PT35A | PCLKT1_0                 |           |
    | B13/1    |     unused, PULL:DOWN |            |               | PT42A |                          |           |
    | B15/1    |     unused, PULL:DOWN |            |               | PT51A |                          |           |
    | B16/1    | gpdi_dp[0]-           |            | LVCMOS33D_OUT | PT56B |                          |           |
    | B17/1    |     unused, PULL:DOWN |            |               | PT60A |                          |           |
    | B18/1    | gpdi_dp[3]-           |            | LVCMOS33D_OUT | PT62B |                          |           |
    | B19/1    |     unused, PULL:DOWN |            |               | PT65B |                          |           |
    | B20/1    |     unused, PULL:DOWN |            |               | PT67B |                          |           |
    | C1/7     | led[2]                | LOCATED    | LVCMOS33_OUT  | PL17A | LDQ20                    |           |
    | C2/7     | led[1]                | LOCATED    | LVCMOS33_OUT  | PL14D | LDQ20                    |           |
    | C3/7     |     unused, PULL:DOWN |            |               | PL8C  | LDQ8                     |           |
    | C4/7     |     unused, PULL:DOWN |            |               | PL5A  | LDQ8                     |           |
    | C5/7     |     unused, PULL:DOWN |            |               | PL2D  | LDQ8                     |           |
    | C6/0     |     unused, PULL:DOWN |            |               | PT11A |                          |           |
    | C7/0     |     unused, PULL:DOWN |            |               | PT11B |                          |           |
    | C8/0     |     unused, PULL:DOWN |            |               | PT15A |                          |           |
    | C10/0    |     unused, PULL:DOWN |            |               | PT22B |                          |           |
    | C11/0    |     unused, PULL:DOWN |            |               | PT29B |                          |           |
    | C12/1    |     unused, PULL:DOWN |            |               | PT35B |                          |           |
    | C13/1    |     unused, PULL:DOWN |            |               | PT42B |                          |           |
    | C14/1    | gpdi_dp[1]-           |            | LVCMOS33D_OUT | PT47B |                          |           |
    | C15/1    |     unused, PULL:DOWN |            |               | PT51B |                          |           |
    | C16/1    |     unused, PULL:DOWN |            |               | PT58A |                          |           |
    | C17/1    |     unused, PULL:DOWN |            |               | PT60B |                          |           |
    | C18/2    |     unused, PULL:DOWN |            |               | PR2A  | RDQ8                     |           |
    | C20/2    |     unused, PULL:DOWN |            |               | PR14A | RDQ20                    |           |
    | CCLK/8   |                       |            |               | CCLK  | MCLK/SCK                 |           |
    | D1/7     | led[4]                | LOCATED    | LVCMOS33_OUT  | PL17B | LDQ20                    |           |
    | D2/7     | led[3]                | LOCATED    | LVCMOS33_OUT  | PL17C | LDQ20                    |           |
    | D3/7     |     unused, PULL:DOWN |            |               | PL8D  | LDQ8                     |           |
    | D5/7     |     unused, PULL:DOWN |            |               | PL8B  | LDQSN8                   |           |
    | D6/0     | btn[0]                | LOCATED    | LVCMOS33_IN   | PT6B  |                          |           |
    | D7/0     |     unused, PULL:DOWN |            |               | PT9B  |                          |           |
    | D8/0     |     unused, PULL:DOWN |            |               | PT13B |                          |           |
    | D9/0     |     unused, PULL:DOWN |            |               | PT20A |                          |           |
    | D11/1    |     unused, PULL:DOWN |            |               | PT33A | PCLKT1_1                 |           |
    | D12/1    |     unused, PULL:DOWN |            |               | PT38A | GR_PCLK1_0               |           |
    | D13/1    |     unused, PULL:DOWN |            |               | PT44A |                          |           |
    | D14/1    |     unused, PULL:DOWN |            |               | PT49A |                          |           |
    | D15/1    |     unused, PULL:DOWN |            |               | PT53A |                          |           |
    | D16/1    |     unused, PULL:DOWN |            |               | PT58B |                          |           |
    | D17/2    |     unused, PULL:DOWN |            |               | PR2B  | S0_IN/RDQ8               |           |
    | D18/2    |     unused, PULL:DOWN |            |               | PR5A  | RDQ8                     |           |
    | D19/2    |     unused, PULL:DOWN |            |               | PR14B | RDQ20                    |           |
    | D20/2    |     unused, PULL:DOWN |            |               | PR14C | VREF1_2/RDQ20            |           |
    | E1/7     | led[6]                | LOCATED    | LVCMOS33_OUT  | PL17D | LDQ20                    |           |
    | E2/7     | led[5]                | LOCATED    | LVCMOS33_OUT  | PL23D | PCLKC7_0/LDQ20           |           |
    | E3/7     |     unused, PULL:DOWN |            |               | PL11B | LDQ8                     |           |
    | E4/7     |     unused, PULL:DOWN |            |               | PL8A  | LDQS8                    |           |
    | E5/7     |     unused, PULL:DOWN |            |               | PL11C | LDQ8                     |           |
    | E6/0     |     unused, PULL:DOWN |            |               | PT6A  |                          |           |
    | E7/0     |     unused, PULL:DOWN |            |               | PT9A  |                          |           |
    | E8/0     |     unused, PULL:DOWN |            |               | PT13A |                          |           |
    | E9/0     |     unused, PULL:DOWN |            |               | PT20B |                          |           |
    | E11/1    |     unused, PULL:DOWN |            |               | PT33B |                          |           |
    | E12/1    |     unused, PULL:DOWN |            |               | PT38B | GR_PCLK1_1               |           |
    | E13/1    |     unused, PULL:DOWN |            |               | PT44B |                          |           |
    | E14/1    |     unused, PULL:DOWN |            |               | PT49B |                          |           |
    | E15/1    |     unused, PULL:DOWN |            |               | PT53B |                          |           |
    | E16/2    |     unused, PULL:DOWN |            |               | PR2C  | RDQ8                     |           |
    | E17/2    |     unused, PULL:DOWN |            |               | PR5B  | RDQ8                     |           |
    | E18/2    |     unused, PULL:DOWN |            |               | PR5C  | RDQ8                     |           |
    | E19/2    |     unused, PULL:DOWN |            |               | PR14D | RDQ20                    |           |
    | E20/2    |     unused, PULL:DOWN |            |               | PR17A | RDQ20                    |           |
    | F1/6     |     unused, PULL:DOWN |            |               | PL26B | PCLKC6_1/LDQ32           |           |
    | F2/7     |     unused, PULL:DOWN |            |               | PL23C | PCLKT7_0/LDQ20           |           |
    | F3/7     |     unused, PULL:DOWN |            |               | PL23B | PCLKC7_1/LDQ20           |           |
    | F4/7     |     unused, PULL:DOWN |            |               | PL11A | LDQ8                     |           |
    | F5/7     |     unused, PULL:DOWN |            |               | PL11D | LDQ8                     |           |
    | F16/2    |     unused, PULL:DOWN |            |               | PR2D  | RDQ8                     |           |
    | F17/2    |     unused, PULL:DOWN |            |               | PR8A  | RDQS8                    |           |
    | F18/2    |     unused, PULL:DOWN |            |               | PR5D  | RDQ8                     |           |
    | F19/2    |     unused, PULL:DOWN |            |               | PR17B | RDQ20                    |           |
    | F20/2    |     unused, PULL:DOWN |            |               | PR17C | RDQ20                    |           |
    | G1/6     |     unused, PULL:DOWN |            |               | PL26D | PCLKC6_0/LDQ32           |           |
    | G2/6     | clk_25mhz             | LOCATED    | LVCMOS33_IN   | PL26A | PCLKT6_1/LDQ32           |           |
    | G3/7     |     unused, PULL:DOWN |            |               | PL23A | PCLKT7_1/LDQ20           |           |
    | G5/7     |     unused, PULL:DOWN |            |               | PL20B | LDQSN20                  |           |
    | G16/2    |     unused, PULL:DOWN |            |               | PR8C  | RDQ8                     |           |
    | G18/2    |     unused, PULL:DOWN |            |               | PR8B  | RDQSN8                   |           |
    | G19/2    |     unused, PULL:DOWN |            |               | PR20A | GR_PCLK2_1/RDQS20        |           |
    | G20/2    |     unused, PULL:DOWN |            |               | PR17D | RDQ20                    |           |
    | H1/6     |     unused, PULL:DOWN |            |               | PL32C | LDQ32                    |           |
    | H2/6     |     unused, PULL:DOWN |            |               | PL26C | PCLKT6_0/LDQ32           |           |
    | H3/7     | led[7]                | LOCATED    | LVCMOS33_OUT  | PL20D | LDQ20                    |           |
    | H4/7     |     unused, PULL:DOWN |            |               | PL20A | GR_PCLK7_1/LDQS20        |           |
    | H5/7     |     unused, PULL:DOWN |            |               | PL20C | GR_PCLK7_0/LDQ20         |           |
    | H16/2    |     unused, PULL:DOWN |            |               | PR8D  | RDQ8                     |           |
    | H17/2    |     unused, PULL:DOWN |            |               | PR11B | RDQ8                     |           |
    | H18/2    |     unused, PULL:DOWN |            |               | PR11A | RDQ8                     |           |
    | H20/2    |     unused, PULL:DOWN |            |               | PR20B | RDQSN20                  |           |
    | J1/6     |     unused, PULL:DOWN |            |               | PL32B | LDQSN32                  |           |
    | J3/6     |     unused, PULL:DOWN |            |               | PL29C | GR_PCLK6_1/LDQ32         |           |
    | J4/6     |     unused, PULL:DOWN |            |               | PL29A | GR_PCLK6_0/LDQ32         |           |
    | J5/6     |     unused, PULL:DOWN |            |               | PL29B | LDQ32                    |           |
    | J16/2    |     unused, PULL:DOWN |            |               | PR11D | RDQ8                     |           |
    | J17/2    |     unused, PULL:DOWN |            |               | PR11C | RDQ8                     |           |
    | J18/2    |     unused, PULL:DOWN |            |               | PR20C | GR_PCLK2_0/RDQ20         |           |
    | J19/2    |     unused, PULL:DOWN |            |               | PR23A | PCLKT2_1/RDQ20           |           |
    | J20/2    |     unused, PULL:DOWN |            |               | PR23C | PCLKT2_0/RDQ20           |           |
    | K1/6     |     unused, PULL:DOWN |            |               | PL32D | LDQ32                    |           |
    | K2/6     |     unused, PULL:DOWN |            |               | PL32A | LDQS32                   |           |
    | K3/6     |     unused, PULL:DOWN |            |               | PL29D | LDQ32                    |           |
    | K4/6     |     unused, PULL:DOWN |            |               | PL35A | LDQ32                    |           |
    | K5/6     |     unused, PULL:DOWN |            |               | PL35B | VREF1_6/LDQ32            |           |
    | K18/2    |     unused, PULL:DOWN |            |               | PR20D | RDQ20                    |           |
    | K19/2    |     unused, PULL:DOWN |            |               | PR23B | PCLKC2_1/RDQ20           |           |
    | K20/2    |     unused, PULL:DOWN |            |               | PR23D | PCLKC2_0/RDQ20           |           |
    | L1/6     |     unused, PULL:DOWN |            |               | PL44C | LDQ44                    |           |
    | L2/6     | wifi_gpio0            | LOCATED    | LVCMOS33_OUT  | PL41D | LDQ44                    |           |
    | L3/6     |     unused, PULL:DOWN |            |               | PL41C | LDQ44                    |           |
    | L4/6     |     unused, PULL:DOWN |            |               | PL35C | LDQ32                    |           |
    | L5/6     |     unused, PULL:DOWN |            |               | PL35D | LDQ32                    |           |
    | L16/3    |     unused, PULL:DOWN |            |               | PR29A | GR_PCLK3_0/RDQ32         |           |
    | L17/3    |     unused, PULL:DOWN |            |               | PR29B | RDQ32                    |           |
    | L18/3    |     unused, PULL:DOWN |            |               | PR29C | GR_PCLK3_1/RDQ32         |           |
    | L19/3    |     unused, PULL:DOWN |            |               | PR26C | PCLKT3_0/RDQ32           |           |
    | L20/3    |     unused, PULL:DOWN |            |               | PR26A | PCLKT3_1/RDQ32           |           |
    | M1/6     |     unused, PULL:DOWN |            |               | PL44B | LDQSN44                  |           |
    | M3/6     |     unused, PULL:DOWN |            |               | PL41B | LDQ44                    |           |
    | M4/6     | user_programn         | LOCATED    | LVCMOS33_OUT  | PL38A | LDQ44                    |           |
    | M17/3    |     unused, PULL:DOWN |            |               | PR32B | RDQSN32                  |           |
    | M18/3    |     unused, PULL:DOWN |            |               | PR29D | RDQ32                    |           |
    | M19/3    |     unused, PULL:DOWN |            |               | PR26D | PCLKC3_0/RDQ32           |           |
    | M20/3    |     unused, PULL:DOWN |            |               | PR26B | PCLKC3_1/RDQ32           |           |
    | N1/6     |     unused, PULL:DOWN |            |               | PL44D | LDQ44                    |           |
    | N2/6     |     unused, PULL:DOWN |            |               | PL44A | LDQS44                   |           |
    | N3/6     |     unused, PULL:DOWN |            |               | PL41A | LDQ44                    |           |
    | N4/6     |     unused, PULL:DOWN |            |               | PL38C | LDQ44                    |           |
    | N5/6     |     unused, PULL:DOWN |            |               | PL38B | LDQ44                    |           |
    | N16/3    |     unused, PULL:DOWN |            |               | PR32A | RDQS32                   |           |
    | N17/3    |     unused, PULL:DOWN |            |               | PR35A | RDQ32                    |           |
    | N18/3    |     unused, PULL:DOWN |            |               | PR32C | RDQ32                    |           |
    | N19/3    |     unused, PULL:DOWN |            |               | PR38A | RDQ44                    |           |
    | N20/3    |     unused, PULL:DOWN |            |               | PR38B | RDQ44                    |           |
    | P1/6     |     unused, PULL:DOWN |            |               | PL47A | LDQ44                    |           |
    | P2/6     |     unused, PULL:DOWN |            |               | PL47B | LDQ44                    |           |
    | P3/6     |     unused, PULL:DOWN |            |               | PL47C | LLC_GPLL0T_IN/LDQ44      |           |
    | P4/6     |     unused, PULL:DOWN |            |               | PL47D | LLC_GPLL0C_IN/LDQ44      |           |
    | P5/6     |     unused, PULL:DOWN |            |               | PL38D | LDQ44                    |           |
    | P16/3    |     unused, PULL:DOWN |            |               | PR35B | VREF1_3/RDQ32            |           |
    | P17/3    |     unused, PULL:DOWN |            |               | PR32D | RDQ32                    |           |
    | P18/3    |     unused, PULL:DOWN |            |               | PR38D | RDQ44                    |           |
    | P19/3    |     unused, PULL:DOWN |            |               | PR38C | RDQ44                    |           |
    | P20/3    |     unused, PULL:DOWN |            |               | PR41A | RDQ44                    |           |
    | PT31A/0  |     unused, PULL:DOWN |            |               |       |                          |           |
    | PT31B/0  |     unused, PULL:DOWN |            |               |       |                          |           |
    | R1/8     |     unused, PULL:DOWN |            |               | PB4A  | D7/IO7                   |           |
    | R2/8     | Reserved: sysCONFIG   |            | LVCMOS33_BIDI | PB15A | HOLDN/DI/BUSY/CSSPIN/CEN |           |
    | R3/8     |     unused, PULL:DOWN |            |               | PB15B | DOUT/CSON                |           |
    | R16/3    |     unused, PULL:DOWN |            |               | PR35C | RDQ32                    |           |
    | R17/3    |     unused, PULL:DOWN |            |               | PR35D | RDQ32                    |           |
    | R18/3    |     unused, PULL:DOWN |            |               | PR44B | RDQSN44                  |           |
    | R20/3    |     unused, PULL:DOWN |            |               | PR41B | RDQ44                    |           |
    | T1/8     |     unused, PULL:DOWN |            |               | PB4B  | D6/IO6                   |           |
    | T2/8     |     unused, PULL:DOWN |            |               | PB13A | SN/CSN                   |           |
    | T3/8     |     unused, PULL:DOWN |            |               | PB18A | WRITEN                   |           |
    | T17/3    |     unused, PULL:DOWN |            |               | PR47D | LRC_GPLL0C_IN/RDQ44      |           |
    | T18/3    |     unused, PULL:DOWN |            |               | PR44D | RDQ44                    |           |
    | T19/3    |     unused, PULL:DOWN |            |               | PR44A | RDQS44                   |           |
    | T20/3    |     unused, PULL:DOWN |            |               | PR41C | RDQ44                    |           |
    | TCK/40   |                       |            |               | TCK   |                          |           |
    | TDI/40   |                       |            |               | TDI   |                          |           |
    | TDO/40   |                       |            |               | TDO   |                          |           |
    | TMS/40   |                       |            |               | TMS   |                          |           |
    | U1/8     |     unused, PULL:DOWN |            |               | PB6A  | D5/MISO2/IO5             |           |
    | U2/8     |     unused, PULL:DOWN |            |               | PB13B | CS1N                     |           |
    | U16/3    |     unused, PULL:DOWN |            |               | PR47C | LRC_GPLL0T_IN/RDQ44      |           |
    | U17/3    |     unused, PULL:DOWN |            |               | PR47B | RDQ44                    |           |
    | U18/3    |     unused, PULL:DOWN |            |               | PR47A | RDQ44                    |           |
    | U19/3    |     unused, PULL:DOWN |            |               | PR44C | RDQ44                    |           |
    | U20/3    |     unused, PULL:DOWN |            |               | PR41D | RDQ44                    |           |
    | V1/8     |     unused, PULL:DOWN |            |               | PB6B  | D4/MOSI2/IO4             |           |
    | V2/8     | Reserved: sysCONFIG   |            | LVCMOS33_BIDI | PB11A | D1/MISO/IO1              |           |
    | W1/8     | Reserved: sysCONFIG   |            | LVCMOS33_BIDI | PB9A  | D3/IO3                   |           |
    | W2/8     | Reserved: sysCONFIG   |            | LVCMOS33_BIDI | PB11B | D0/MOSI/IO0              |           |
    | Y2/8     | Reserved: sysCONFIG   |            | LVCMOS33_BIDI | PB9B  | D2/IO2                   |           |
    +----------+-----------------------+------------+---------------+-------+--------------------------+-----------+

    Shared Persistent sysCONFIG Pins:
    +----------+--------------------------+------------------------+----------+---------------+-------------------+
    | Pad Name | sysCONFIG Pin Name       | sysCONFIG Settings     | Pin/Bank | Buffer Type   | Config Pull Mode  |
    +----------+--------------------------+------------------------+----------+---------------+-------------------+
    | PB9A     | D3/IO3                   | MASTER_SPI_PORT=ENABLE | W1/8     | LVCMOS33_BIDI | NO pull up/down   |
    | PB11A    | D1/MISO/IO1              | MASTER_SPI_PORT=ENABLE | V2/8     | LVCMOS33_BIDI | NO pull up/down   |
    | PB9B     | D2/IO2                   | MASTER_SPI_PORT=ENABLE | Y2/8     | LVCMOS33_BIDI | NO pull up/down   |
    | PB11B    | D0/MOSI/IO0              | MASTER_SPI_PORT=ENABLE | W2/8     | LVCMOS33_BIDI | NO pull up/down   |
    | PB15A    | HOLDN/DI/BUSY/CSSPIN/CEN | MASTER_SPI_PORT=ENABLE | R2/8     | LVCMOS33_BIDI | PULLUP            |
    +----------+--------------------------+------------------------+----------+---------------+-------------------+

    Dedicated sysCONFIG Pins:
    +----------+--------------------+------------------------+
    | Pin/Bank | sysCONFIG Pin Name | sysCONFIG Settings     |
    +----------+--------------------+------------------------+
    | V3/8     | INITN              | MASTER_SPI_PORT=ENABLE |
    | U3/8     | MCLK/SCK           | MASTER_SPI_PORT=ENABLE |
    | W3/8     | PROGRAMN           | MASTER_SPI_PORT=ENABLE |
    | Y3/8     | DONE               | MASTER_SPI_PORT=ENABLE |
    | T4/8     | CFG_1              | MASTER_SPI_PORT=ENABLE |
    | R4/8     | CFG_2              | MASTER_SPI_PORT=ENABLE |
    | U4/8     | CFG_0              | MASTER_SPI_PORT=ENABLE |
    +----------+--------------------+------------------------+

    List of All Pins' Locate Preferences Based on Final Placement After PAR
    to Help Users Lock Down ALL the Pins Easily (by Simply Copy & Paste):

    LOCATE  COMP  "btn[0]"  SITE  "D6";
    LOCATE  COMP  "clk_25mhz"  SITE  "G2";
    LOCATE  COMP  "gpdi_dp[0]"  SITE  "A16";
    LOCATE  COMP  "gpdi_dp[1]"  SITE  "A14";
    LOCATE  COMP  "gpdi_dp[2]"  SITE  "A12";
    LOCATE  COMP  "gpdi_dp[3]"  SITE  "A17";
    LOCATE  COMP  "led[0]"  SITE  "B2";
    LOCATE  COMP  "led[1]"  SITE  "C2";
    LOCATE  COMP  "led[2]"  SITE  "C1";
    LOCATE  COMP  "led[3]"  SITE  "D2";
    LOCATE  COMP  "led[4]"  SITE  "D1";
    LOCATE  COMP  "led[5]"  SITE  "E2";
    LOCATE  COMP  "led[6]"  SITE  "E1";
    LOCATE  COMP  "led[7]"  SITE  "H3";
    LOCATE  COMP  "user_programn"  SITE  "M4";
    LOCATE  COMP  "wifi_gpio0"  SITE  "L2";

    #PLL
    LOCATE  COMP  "PLL1_inst/PLLInst_0"  SITE  "PLL_BL0" ;

    PAR: Place And Route Diamond (64-bit) 3.12.1.454.
    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995 AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems   All rights reserved.
    Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.
    Sun Dec 05 13:18:12 2021