    Place & Route TRACE Report

    Loading design for application trce from file blink_p2_a2_impl.ncd.
    Design name: TinyFPGA_A2
    NCD version: 3.3
    Vendor:      LATTICE
    Device:      LCMXO2-1200HC
    Package:     QFN32
    Performance: 4
    Loading device for application trce from file 'xo2c1200.nph' in environment: C:/lscc/diamond/3.12/ispfpga.
    Package Status:                     Final          Version 1.44.
    Performance Hardware Data Status:   Final          Version 34.4.
    Setup and Hold Report

    --------------------------------------------------------------------------------
    Lattice TRACE Report - Setup, Version Diamond (64-bit) 3.12.1.454
    Mon Nov 08 11:09:51 2021

    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995 AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems   All rights reserved.
    Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.

    Report Information
    ------------------
    Command line:    trce -v 10 -gt -sethld -sp 4 -sphld m -o Blink_P2_a2_impl.twr -gui -msgset C:/FPGA/AdderProject/promote.xml Blink_P2_a2_impl.ncd Blink_P2_a2_impl.prf
    Design file:     blink_p2_a2_impl.ncd
    Preference file: blink_p2_a2_impl.prf
    Device,speed:    LCMXO2-1200HC,4
    Report level:    verbose report, limited to 10 items per preference
    --------------------------------------------------------------------------------

    Preference Summary

    Default path enumeration(0 errors)            28 items scored, 0 timing errors detected.

    Default net enumeration(0 errors)            16 items scored, 0 timing errors detected.

    BLOCK ASYNCPATHS
    BLOCK RESETPATHS
    --------------------------------------------------------------------------------

    ================================================================================
    Preference: Default path enumeration
                28 items scored, 0 timing errors detected.
    --------------------------------------------------------------------------------

    Report:   12.668ns delay p2pin8 to p2pin4

       Name    Fanout   Delay (ns)          Site               Resource
    PADI_DEL    ---     1.372         28.PAD to       28.PADDI p2pin8
    ROUTE         3     3.034       28.PADDI to     R10C11B.A1 p2pin8_c
    CTOF_DEL    ---     0.495     R10C11B.A1 to     R10C11B.F1 SLICE_1
    ROUTE         2     0.445     R10C11B.F1 to     R10C11D.C1 n92
    CTOF_DEL    ---     0.495     R10C11D.C1 to     R10C11D.F1 SLICE_0
    ROUTE         2     0.445     R10C11D.F1 to     R10C11D.C0 n91
    CTOF_DEL    ---     0.495     R10C11D.C0 to     R10C11D.F0 SLICE_0
    ROUTE         1     2.439     R10C11D.F0 to       20.PADDO p2pin4_c
    DOPAD_DEL   ---     3.448       20.PADDO to         20.PAD p2pin4
                      --------
                       12.668   (49.8% logic, 50.2% route), 5 logic levels.

    Report:   12.609ns delay p2pin8 to p2pin3

       Name    Fanout   Delay (ns)          Site               Resource
    PADI_DEL    ---     1.372         28.PAD to       28.PADDI p2pin8
    ROUTE         3     3.034       28.PADDI to     R10C11B.A1 p2pin8_c
    CTOF_DEL    ---     0.495     R10C11B.A1 to     R10C11B.F1 SLICE_1
    ROUTE         2     0.445     R10C11B.F1 to     R10C11D.C1 n92
    CTOF_DEL    ---     0.495     R10C11D.C1 to     R10C11D.F1 SLICE_0
    ROUTE         2     0.756     R10C11D.F1 to     R10C11A.C0 n91
    CTOF_DEL    ---     0.495     R10C11A.C0 to     R10C11A.F0 SLICE_3
    ROUTE         1     2.069     R10C11A.F0 to       17.PADDO p2pin3_c
    DOPAD_DEL   ---     3.448       17.PADDO to         17.PAD p2pin3
                      --------
                       12.609   (50.0% logic, 50.0% route), 5 logic levels.

    Report:   12.436ns delay p2pin9 to p2pin4

       Name    Fanout   Delay (ns)          Site               Resource
    PADI_DEL    ---     1.372          4.PAD to        4.PADDI p2pin9
    ROUTE         2     2.802        4.PADDI to     R10C11B.C1 p2pin9_c
    CTOF_DEL    ---     0.495     R10C11B.C1 to     R10C11B.F1 SLICE_1
    ROUTE         2     0.445     R10C11B.F1 to     R10C11D.C1 n92
    CTOF_DEL    ---     0.495     R10C11D.C1 to     R10C11D.F1 SLICE_0
    ROUTE         2     0.445     R10C11D.F1 to     R10C11D.C0 n91
    CTOF_DEL    ---     0.495     R10C11D.C0 to     R10C11D.F0 SLICE_0
    ROUTE         1     2.439     R10C11D.F0 to       20.PADDO p2pin4_c
    DOPAD_DEL   ---     3.448       20.PADDO to         20.PAD p2pin4
                      --------
                       12.436   (50.7% logic, 49.3% route), 5 logic levels.

    Report:   12.377ns delay p2pin9 to p2pin3

       Name    Fanout   Delay (ns)          Site               Resource
    PADI_DEL    ---     1.372          4.PAD to        4.PADDI p2pin9
    ROUTE         2     2.802        4.PADDI to     R10C11B.C1 p2pin9_c
    CTOF_DEL    ---     0.495     R10C11B.C1 to     R10C11B.F1 SLICE_1
    ROUTE         2     0.445     R10C11B.F1 to     R10C11D.C1 n92
    CTOF_DEL    ---     0.495     R10C11D.C1 to     R10C11D.F1 SLICE_0
    ROUTE         2     0.756     R10C11D.F1 to     R10C11A.C0 n91
    CTOF_DEL    ---     0.495     R10C11A.C0 to     R10C11A.F0 SLICE_3
    ROUTE         1     2.069     R10C11A.F0 to       17.PADDO p2pin3_c
    DOPAD_DEL   ---     3.448       17.PADDO to         17.PAD p2pin3
                      --------
                       12.377   (50.9% logic, 49.1% route), 5 logic levels.

    Report:   12.205ns delay p2pin13 to p2pin4

       Name    Fanout   Delay (ns)          Site               Resource
    PADI_DEL    ---     1.372         10.PAD to       10.PADDI p2pin13
    ROUTE         2     2.571       10.PADDI to     R10C11B.B1 p2pin13_c
    CTOF_DEL    ---     0.495     R10C11B.B1 to     R10C11B.F1 SLICE_1
    ROUTE         2     0.445     R10C11B.F1 to     R10C11D.C1 n92
    CTOF_DEL    ---     0.495     R10C11D.C1 to     R10C11D.F1 SLICE_0
    ROUTE         2     0.445     R10C11D.F1 to     R10C11D.C0 n91
    CTOF_DEL    ---     0.495     R10C11D.C0 to     R10C11D.F0 SLICE_0
    ROUTE         1     2.439     R10C11D.F0 to       20.PADDO p2pin4_c
    DOPAD_DEL   ---     3.448       20.PADDO to         20.PAD p2pin4
                      --------
                       12.205   (51.7% logic, 48.3% route), 5 logic levels.

    Report:   12.146ns delay p2pin13 to p2pin3

       Name    Fanout   Delay (ns)          Site               Resource
    PADI_DEL    ---     1.372         10.PAD to       10.PADDI p2pin13
    ROUTE         2     2.571       10.PADDI to     R10C11B.B1 p2pin13_c
    CTOF_DEL    ---     0.495     R10C11B.B1 to     R10C11B.F1 SLICE_1
    ROUTE         2     0.445     R10C11B.F1 to     R10C11D.C1 n92
    CTOF_DEL    ---     0.495     R10C11D.C1 to     R10C11D.F1 SLICE_0
    ROUTE         2     0.756     R10C11D.F1 to     R10C11A.C0 n91
    CTOF_DEL    ---     0.495     R10C11A.C0 to     R10C11A.F0 SLICE_3
    ROUTE         1     2.069     R10C11A.F0 to       17.PADDO p2pin3_c
    DOPAD_DEL   ---     3.448       17.PADDO to         17.PAD p2pin3
                      --------
                       12.146   (51.9% logic, 48.1% route), 5 logic levels.

    Report:   11.716ns delay p2pin10 to p2pin4

       Name    Fanout   Delay (ns)          Site               Resource
    PADI_DEL    ---     1.372          5.PAD to        5.PADDI p2pin10
    ROUTE         2     3.022        5.PADDI to     R10C11D.A1 p2pin10_c
    CTOF_DEL    ---     0.495     R10C11D.A1 to     R10C11D.F1 SLICE_0
    ROUTE         2     0.445     R10C11D.F1 to     R10C11D.C0 n91
    CTOF_DEL    ---     0.495     R10C11D.C0 to     R10C11D.F0 SLICE_0
    ROUTE         1     2.439     R10C11D.F0 to       20.PADDO p2pin4_c
    DOPAD_DEL   ---     3.448       20.PADDO to         20.PAD p2pin4
                      --------
                       11.716   (49.6% logic, 50.4% route), 4 logic levels.

    Report:   11.709ns delay p2pin12 to p2pin4

       Name    Fanout   Delay (ns)          Site               Resource
    PADI_DEL    ---     1.372          9.PAD to        9.PADDI p2pin12
    ROUTE         3     2.075        9.PADDI to     R10C11B.D1 p2pin12_c
    CTOF_DEL    ---     0.495     R10C11B.D1 to     R10C11B.F1 SLICE_1
    ROUTE         2     0.445     R10C11B.F1 to     R10C11D.C1 n92
    CTOF_DEL    ---     0.495     R10C11D.C1 to     R10C11D.F1 SLICE_0
    ROUTE         2     0.445     R10C11D.F1 to     R10C11D.C0 n91
    CTOF_DEL    ---     0.495     R10C11D.C0 to     R10C11D.F0 SLICE_0
    ROUTE         1     2.439     R10C11D.F0 to       20.PADDO p2pin4_c
    DOPAD_DEL   ---     3.448       20.PADDO to         20.PAD p2pin4
                      --------
                       11.709   (53.8% logic, 46.2% route), 5 logic levels.

    Report:   11.657ns delay p2pin10 to p2pin3

       Name    Fanout   Delay (ns)          Site               Resource
    PADI_DEL    ---     1.372          5.PAD to        5.PADDI p2pin10
    ROUTE         2     3.022        5.PADDI to     R10C11D.A1 p2pin10_c
    CTOF_DEL    ---     0.495     R10C11D.A1 to     R10C11D.F1 SLICE_0
    ROUTE         2     0.756     R10C11D.F1 to     R10C11A.C0 n91
    CTOF_DEL    ---     0.495     R10C11A.C0 to     R10C11A.F0 SLICE_3
    ROUTE         1     2.069     R10C11A.F0 to       17.PADDO p2pin3_c
    DOPAD_DEL   ---     3.448       17.PADDO to         17.PAD p2pin3
                      --------
                       11.657   (49.8% logic, 50.2% route), 4 logic levels.

    Report:   11.650ns delay p2pin12 to p2pin3

       Name    Fanout   Delay (ns)          Site               Resource
    PADI_DEL    ---     1.372          9.PAD to        9.PADDI p2pin12
    ROUTE         3     2.075        9.PADDI to     R10C11B.D1 p2pin12_c
    CTOF_DEL    ---     0.495     R10C11B.D1 to     R10C11B.F1 SLICE_1
    ROUTE         2     0.445     R10C11B.F1 to     R10C11D.C1 n92
    CTOF_DEL    ---     0.495     R10C11D.C1 to     R10C11D.F1 SLICE_0
    ROUTE         2     0.756     R10C11D.F1 to     R10C11A.C0 n91
    CTOF_DEL    ---     0.495     R10C11A.C0 to     R10C11A.F0 SLICE_3
    ROUTE         1     2.069     R10C11A.F0 to       17.PADDO p2pin3_c
    DOPAD_DEL   ---     3.448       17.PADDO to         17.PAD p2pin3
                      --------
                       11.650   (54.1% logic, 45.9% route), 5 logic levels.

    Report:   12.668ns is the maximum delay for this preference.

    ================================================================================
    Preference: Default net enumeration
                16 items scored, 0 timing errors detected.
    --------------------------------------------------------------------------------

    Report:    4.216ns maximum delay on GND_net

               Delays             Connection(s)
               4.216ns       R10C11A.F1 to 27.PADDO
               3.720ns       R10C11A.F1 to 26.PADDO
               3.720ns       R10C11A.F1 to 25.PADDO
               2.852ns       R10C11A.F1 to 23.PADDO
               2.750ns       R10C11A.F1 to 21.PADDO

    Report:    3.483ns maximum delay on p2pin8_c

               Delays             Connection(s)
               3.483ns         28.PADDI to R10C11C.B1
               3.483ns         28.PADDI to R10C11C.B0
               3.034ns         28.PADDI to R10C11B.A1

    Report:    3.078ns maximum delay on p2pin10_c

               Delays             Connection(s)
               3.078ns          5.PADDI to R10C11B.D0
               3.022ns          5.PADDI to R10C11D.A1

    Report:    2.802ns maximum delay on p2pin9_c

               Delays             Connection(s)
               2.802ns          4.PADDI to R10C11C.C0
               2.802ns          4.PADDI to R10C11B.C1

    Report:    2.590ns maximum delay on p2pin11_c

               Delays             Connection(s)
               2.590ns          8.PADDI to R10C11A.D0
               2.193ns          8.PADDI to R10C11D.D0

    Report:    2.571ns maximum delay on p2pin13_c

               Delays             Connection(s)
               2.534ns         10.PADDI to R10C11C.A0
               2.571ns         10.PADDI to R10C11B.B1

    Report:    2.439ns maximum delay on p2pin4_c

               Delays             Connection(s)
               2.439ns       R10C11D.F0 to 20.PADDO

    Report:    2.235ns maximum delay on p2pin2_c

               Delays             Connection(s)
               2.235ns       R10C11B.F0 to 16.PADDO

    Report:    2.075ns maximum delay on p2pin12_c

               Delays             Connection(s)
               2.075ns          9.PADDI to R10C11C.D1
               2.075ns          9.PADDI to R10C11C.D0
               2.075ns          9.PADDI to R10C11B.D1

    Report:    2.069ns maximum delay on p2pin3_c

               Delays             Connection(s)
               2.069ns       R10C11A.F0 to 17.PADDO

    Report:    4.216ns is the maximum delay for this preference.

    Report Summary
    --------------
    ----------------------------------------------------------------------------
    Preference                              |   Constraint|       Actual|Levels
    ----------------------------------------------------------------------------
                                            |             |             |
    Default path enumeration                |     0.000 ns|    12.668 ns|   0
                                            |             |             |
    Default net enumeration                 |     0.000 ns|     4.216 ns|   0
                                            |             |             |
    ----------------------------------------------------------------------------

    All preferences were met.

    Clock Domains Analysis
    ------------------------

    Found 0 clocks:

    Timing summary (Setup):
    ---------------

    Timing errors: 0  Score: 0
    Cumulative negative slack: 0

    Constraints cover 28 paths, 16 nets, and 32 connections (100.00% coverage)

    --------------------------------------------------------------------------------